/\* File: pwm8bits.c

\* Author: Craig Bacon

\* Created on 30 October 2014, 14:11

\* PWM pin 13 right hand motor, mark space ratio is 8 bit (255) and the PWM

\* frequency is 610 Hz PWM Period = (PR2+1)x4 x 1/Osc x TMR2 Prescaler

\* e.g (255+1)x4 x1/10Mhz x 16 =1.638ms or 610Hz.PR2 changes frequency.

\*

\* Need to control pins 13(CCP1) 21(RB0) and 22(RB1)

\*/

#include <xc.h>

#include <stdio.h>

#include <stdlib.h>

#pragma config OSC = HS

#pragma config WDT = OFF

#pragma config LVP = OFF

#pragma config PWRT = ON

#define RA4 LATAbits.LATA4

#define RA5 LATAbits.LATA5

int main(void)

{

int markspace=127; //mark space value for 8 PWM (50% mark space ratio)

TRISCbits.RC1=0; //set CCP1(pin13) to an output pin

TRISA = 0b11000000;

PR2 = 0b11111111 ; //set period of PWM

T2CON = 0b00000111 ; //Timer 2(TMR2) on, Prescaler = 16

CCP2CON = 0b00001100; //0x0c enables PWM module CCP1

CCPR2L = markspace; //Load duty cycle into CCP1CON, PWM begins

while(1){

RA4 = 0;

RA5 = 1;

};

} //end main()